|RECORD=BOM|VERSION=6|FILENAME=D:\work\workspace\altium\templates\template-altium-project\source\BOM\BOM.$$$|KIND=ALTIUM_DESIGNER_LIVEBOM|DATE=20.12.2024|TIME=14:03:34|CURRENCY=USD|PRODUCTIONQUANTITY=1|PERUNITTARGETPRICE=0|PERUNITACTUALPRICE=0
|RECORD=GeneralOptions|OPENEXPORTED=False|ADDTOPROJECT=False|FORCEFIT=False|NOTFITTED=True|TEMPLATEFILENAME=|BATCHMODE=0|SUPPLIERPRODQTY=0|SUPPLIERAUTOQTY=False|SUPPLIERUSECACHEDPRICING=False|SUPPLIERCURRENCY=|SOLUTIONSPERITEM=1|SUPPLIERSPERSOLUTION=1|DISPLAYTOTALROW=False|DISPLAYSUBTOTALSFORGROUPS=False|INCLUDEPCBPARAMETERS=False|INCLUDEDBPARAMETERS=False|INCLUDEVAULTPARAMETERS=False|INCLUDECLOUDPARAMETERS=False|INCLUDEDOCUMENTPARAMETERS=True|FILTEROUTRISKYSOLUTIONS=True|DESIGNATORGROUPING=No
|RECORD=SortOrderOptions|SORTORDER=
|RECORD=GroupOrderOptions|GROUPORDER=
|RECORD=VisibleOrderOptions|VISIBLEORDER=Designator=80!Fitted=77!Part Number=223!Manufacturer=163!Note=50
|RECORD=VisibleOrderOptions2|BASEVIEW=Designator=170!Manufacturer=163!Part Number=223!Fitted=77!Quantity=97|FLATVIEW=Designator=80!Fitted=77!Part Number=223!Manufacturer=163!Note=50|CONSOLIDATEDVIEW=Line #=-1!Comment=-1!Description=-1!Designator=-1!Quantity=-1!Fitted=-1!Manufacturer 1=102!Manufacturer Part Number 1=169!Manufacturer Lifecycle 1=147!Supplier 1=75!Supplier Part Number 1=142!Supplier Unit Price 1=127!Supplier Subtotal 1=122!Quantity@GENERAL=-1!Price@GENERAL=-1
|RECORD=CustomColumns|CUSTOMCOLUMNS=Size=91!Zone=120!Item=210
|RECORD=ColumnsAliases|COLUMNSALIASES=Quantity@00=00 - Qty!Price@00=00 - Price!Quantity@-01=-01 - Qty!Price@-01=-01 - Price!Quantity@PRODUCTION=PRODUCTION - Qty!Price@PRODUCTION=PRODUCTION - Price!Quantity@GENERAL=GENERAL - Qty!Price@GENERAL=GENERAL - Price!Format=Ôîðìàò
|RECORD=FilterOptions|FILTER=
|RECORD=CheckGroupCompParamsOptions|CHECKGROUPCOMPPARAMS=ID=1,Fitted=0
|RECORD=ManufacturerLinkOptions|MANUFACTURERLINKPARAMETERS=Manufacturer=Part Number
|RECORD=FavoriteSuppliers|PARTSOURCES=|SUPPLIERS=LCSC!TME!Digi-Key!Rs!Conrad|USESUPPLIERORDER=True
|RECORD=CheckOptions|CHECKLEVELS=
|RECORD=ExternalCheckOptions|CHECKLEVELS=
|RECORD=LineNumberingOptions|STARTVALUE=1|INCREMENT=1
|RECORD=BOMSet|NAME=BOM|VIEWMODE=Base|SORTORDER=Designator,Ascending|BASECOLUMN=Line #,43~Fitted,63~Designator,170~Quantity,97~Database Table Name,133~Description,256~Manufacturer,163~Part Number,108~Value,110~Notes,133|FLATCOLUMN=Line #,~Comment,~Description,294~Designator,80~Fitted,~Manufacturer 1,102~Manufacturer Part Number 1,169~Manufacturer Lifecycle 1,147~Supplier 1,75~Supplier Part Number 1,142~Supplier Unit Price 1,127~Supplier Subtotal 1,122|CONSOLIDATEDCOLUMN=Line #,~Comment,~Description,~Designator,~Quantity,~Fitted,~Manufacturer 1,102~Manufacturer Part Number 1,169~Manufacturer Lifecycle 1,147~Supplier 1,75~Supplier Part Number 1,142~Supplier Unit Price 1,127~Supplier Subtotal 1,122~Quantity@GENERAL,~Price@GENERAL,|SHOWNOTFITTED=True
|RECORD=BOMSet|NAME=ORDER LIST|VIEWMODE=Base|SORTORDER=Designator,Ascending|BASECOLUMN=Line #,43~Designator,170~Quantity,97~Database Table Name,133~Description,256~Manufacturer,163~Part Number,108~Value,110~Pins,45~Notes,133~Manufacturer 1,102~Manufacturer Part Number 1,169~Manufacturer Lifecycle 1,147~Supplier 1,75~Supplier Part Number 1,142~Supplier Unit Price 1,127~Supplier Subtotal 1,122|FLATCOLUMN=Line #,~Comment,~Description,~Designator,~Manufacturer 1,102~Manufacturer Part Number 1,169~Manufacturer Lifecycle 1,147~Supplier 1,75~Supplier Part Number 1,142~Supplier Unit Price 1,127~Supplier Subtotal 1,122|CONSOLIDATEDCOLUMN=Line #,~Comment,~Description,~Designator,~Quantity,~Manufacturer 1,102~Manufacturer Part Number 1,169~Manufacturer Lifecycle 1,147~Supplier 1,75~Supplier Part Number 1,142~Supplier Unit Price 1,127~Supplier Subtotal 1,122~Quantity@GENERAL,~Price@GENERAL,|SHOWNOTFITTED=False
|RECORD=BOMSet|NAME=REVIEW|VIEWMODE=Flat|SORTORDER=Designator,Ascending|BASECOLUMN=Designator,170~Quantity,97~Description,256~Manufacturer,163~Partnumber,165~Notes,133~Manufacturer 1,102~Manufacturer Part Number 1,169~Manufacturer Lifecycle 1,147~Supplier 1,75~Supplier Part Number 1,142~Supplier Unit Price 1,127~Supplier Subtotal 1,122|FLATCOLUMN=Designator,80~Component Kind,110~PhysicalPath,194~Database Table Name,133~Description,294~Manufacturer,163~Part Number,108~Notes,133~Manufacturer 1,102~Manufacturer Part Number 1,169~Manufacturer Lifecycle 1,147~Supplier 1,75~Supplier Part Number 1,142~Supplier Unit Price 1,127~Supplier Subtotal 1,122|CONSOLIDATEDCOLUMN=Line #,~Comment,~Description,~Designator,~Quantity,~Manufacturer 1,102~Manufacturer Part Number 1,169~Manufacturer Lifecycle 1,147~Supplier 1,75~Supplier Part Number 1,142~Supplier Unit Price 1,127~Supplier Subtotal 1,122~Quantity@GENERAL,~Price@GENERAL,|SHOWNOTFITTED=False
|RECORD=BOMSet|NAME=GOSTDocTool|VIEWMODE=Flat|SORTORDER=|BASECOLUMN=Designator,170~Manufacturer,163~Part Number,223~Fitted,77~Quantity,97|FLATCOLUMN=Designator,80~Fitted,77~Part Number,223~Manufacturer,163~Note,50|CONSOLIDATEDCOLUMN=Line #,~Comment,~Description,~Designator,~Quantity,~Fitted,~Manufacturer 1,102~Manufacturer Part Number 1,169~Manufacturer Lifecycle 1,147~Supplier 1,75~Supplier Part Number 1,142~Supplier Unit Price 1,127~Supplier Subtotal 1,122~Quantity@GENERAL,~Price@GENERAL,|FLATFILTER=|SHOWNOTFITTED=True
|RECORD=Catalog|DBLINKFILEPATH=
|RECORD=CatalogItem|ITEMTYPE=Automatic-NonVault|UNIQUEID=GhOST Lib.DbLib/LEDs.txt\FORYARD.FYLS-0603URC|DESIGNITEMID=FORYARD.FYLS-0603URC|ITEMSOURCE=GhOST Lib.DbLib/LEDs.txt|STATUS=Unknown|DESCRIPTION=LED RED, SMD 0603, 80mcd|USERCOMMENTS=DIODE_LED|NOTE=|LINENUMBER=2|SELECTEDPARAMETERSHASH=|COMPONENTPARAMETERS="Caption=""DIODE_LED""","Category=Low Power",Color=Red,Comment=DIODE_LED,"Component Kind=Standard",Current=20mA,"Database Table Name=LEDs.txt","Description=LED RED, SMD 0603, 80mcd","Direction=Top View",Footprint=LEDC1608X80N_RED,HelpURL=http://www.foryard-led.ru/pdf/fyls-0603urc.pdf,"Ibis Model=",ID=FORYARD.FYLS-0603URC,"Library Name=GhOST Lib.DbLib","Library Reference=FORYARD.FYLS-0603URC",Manufacturer=FORYARD,Note=,Package=0603,"Part Number=FYLS-0603URC",PCB3D=,"Pin Info=","Signal Integrity=",Simulation=,"Temperature Max=+85","Temperature Min=-40",Voltage=2.6V|CUSTOMPARAMETERS=
|RECORD=PartChoiceGroups|GROUPBYFIELDCOUNT=0
|RECORD=CatalogItem|ITEMTYPE=Automatic-NonVault|UNIQUEID=GhOST Lib.DbLib/LEDs.txt\FORYARD.FYLS-0603UBC|DESIGNITEMID=FORYARD.FYLS-0603UBC|ITEMSOURCE=GhOST Lib.DbLib/LEDs.txt|STATUS=Unknown|DESCRIPTION=LED BLUE, SMD 0603, 120mcd|USERCOMMENTS=DIODE_LED|NOTE=|LINENUMBER=3|SELECTEDPARAMETERSHASH=|COMPONENTPARAMETERS="Caption=""DIODE_LED""","Category=Low Power",Color=Blue,Comment=DIODE_LED,"Component Kind=Standard",Current=20mA,"Database Table Name=LEDs.txt","Description=LED BLUE, SMD 0603, 120mcd","Direction=Top View",Footprint=LEDC1608X80N_BLUE,HelpURL=http://www.foryard-led.ru/pdf/fyls-0603ubc.pdf,"Ibis Model=",ID=FORYARD.FYLS-0603UBC,"Library Name=GhOST Lib.DbLib","Library Reference=FORYARD.FYLS-0603UBC",Manufacturer=FORYARD,Note=,Package=0603,"Part Number=FYLS-0603UBC",PCB3D=,"Pin Info=","Signal Integrity=",Simulation=,"Temperature Max=+85","Temperature Min=-40",Voltage=3.6V|CUSTOMPARAMETERS=
|RECORD=PartChoiceGroups|GROUPBYFIELDCOUNT=0
|RECORD=CatalogItem|ITEMTYPE=Automatic-NonVault|UNIQUEID=GhOST Lib.DbLib/Transistors.txt\ÀÄÊÁ.432140.556 ÒÓ.ÊÒ231Á9|DESIGNITEMID=ÀÄÊÁ.432140.556 ÒÓ.ÊÒ231Á9|ITEMSOURCE=GhOST Lib.DbLib/Transistors.txt|STATUS=Unknown|DESCRIPTION=Òðàíçèñòîð NPN, 0.1À, 45Â, h21e=110…220, ÊÒ-46/SOT-23|USERCOMMENTS=ÊÒ231Á9|NOTE=|LINENUMBER=6|SELECTEDPARAMETERSHASH=|COMPONENTPARAMETERS=Category=Bipolar\NPN,Comment=ÊÒ231Á9,"Component Kind=Standard",Current=100mA,"Database Table Name=Transistors.txt","Description=Òðàíçèñòîð NPN, 0.1À, 45Â, h21e=110…220, ÊÒ-46/SOT-23",Footprint=SOT23-3N,HelpURL=https://group-kremny.ru/upload/iblock/ac4/ac4d75a22fe00fe78de4a89ebc6afcf4.pdf,"Ibis Model=","ID=ÀÄÊÁ.432140.556 ÒÓ.ÊÒ231Á9","Library Name=GhOST Lib.DbLib","Library Reference=ÀÄÊÁ.432140.556 ÒÓ.ÊÒ231Á9","Manufacturer=ÀÄÊÁ.432140.556 ÒÓ","Note=aka BC847A",Package=SOT23-3,"Part Number=ÊÒ231Á9",PCB3D=,"Pin Info=","Signal Integrity=",Simulation=,"Temperature Max=+150","Temperature Min=-65",Voltage=45V|CUSTOMPARAMETERS=
|RECORD=PartChoiceGroups|GROUPBYFIELDCOUNT=0
|RECORD=CatalogItem|ITEMTYPE=Automatic-NonVault|UNIQUEID=GhOST Lib.DbLib/Capacitors.txt\CAPC0805 1U 10% 6.3V X7R|DESIGNITEMID=CAPC0805 1U 10% 6.3V X7R|ITEMSOURCE=GhOST Lib.DbLib/Capacitors.txt|STATUS=Unknown|DESCRIPTION=Chip Ceramic Capacitor SMD 0805 1uF 10% 6.3V X7R|USERCOMMENTS=1u|NOTE=|LINENUMBER=1|SELECTEDPARAMETERSHASH=|COMPONENTPARAMETERS="Category=Chip Ceramic",Comment=1u,"Component Kind=Standard","Database Table Name=Capacitors.txt","Description=Chip Ceramic Capacitor SMD 0805 1uF 10% 6.3V X7R",Footprint=CAPC2012X125N,HelpURL=,"Ibis Model=","ID=CAPC0805 1U 10% 6.3V X7R","Library Name=GhOST Lib.DbLib","Library Reference=CAPC0805 1U 10% 6.3V X7R",Manufacturer=,Material=X7R,Note=,Package=0805,"Part Number=CAPC0805 1U 10% 6.3V X7R",PCB3D=,"Pin Info=","Signal Integrity=",Simulation=,"Temperature Max=","Temperature Min=",Tolerance=10%,Value=1u,Voltage=6.3V|CUSTOMPARAMETERS=
|RECORD=PartChoiceGroups|GROUPBYFIELDCOUNT=0
|RECORD=CatalogItem|ITEMTYPE=Automatic-NonVault|UNIQUEID=GhOST Lib.DbLib/Resistors.txt\RESC0805 470 1%|DESIGNITEMID=RESC0805 470 1%|ITEMSOURCE=GhOST Lib.DbLib/Resistors.txt|STATUS=Unknown|DESCRIPTION=Chip Resistor SMD 0805 470 Ohm 1%|USERCOMMENTS=470|NOTE=|LINENUMBER=4|SELECTEDPARAMETERSHASH=|COMPONENTPARAMETERS=Comment=470,"Component Kind=Standard","Database Table Name=Resistors.txt","Description=Chip Resistor SMD 0805 470 Ohm 1%",Footprint=RESC2012X70N,HelpURL=,"Ibis Model=","ID=RESC0805 470 1%","Library Name=GhOST Lib.DbLib","Library Reference=RESC0805 470 1%",Manufacturer=,Note=,Package=0805,"Part Number=RESC0805 470 1%",PCB3D=,"Pin Info=","Signal Integrity=",Simulation=,TCR=,"Temperature Max=","Temperature Min=",Tolerance=1%,Value=470|CUSTOMPARAMETERS=
|RECORD=PartChoiceGroups|GROUPBYFIELDCOUNT=0
|RECORD=CatalogItem|ITEMTYPE=Automatic-NonVault|UNIQUEID=GhOST Lib.DbLib/Resistors.txt\RESC0805 10K 1%|DESIGNITEMID=RESC0805 10K 1%|ITEMSOURCE=GhOST Lib.DbLib/Resistors.txt|STATUS=Unknown|DESCRIPTION=Chip Resistor SMD 0805 10 kOhm 1%|USERCOMMENTS=10k|NOTE=|LINENUMBER=5|SELECTEDPARAMETERSHASH=|COMPONENTPARAMETERS=Comment=10k,"Component Kind=Standard","Database Table Name=Resistors.txt","Description=Chip Resistor SMD 0805 10 kOhm 1%",Footprint=RESC2012X70N,HelpURL=,"Ibis Model=","ID=RESC0805 10K 1%","Library Name=GhOST Lib.DbLib","Library Reference=RESC0805 10K 1%",Manufacturer=,Note=,Package=0805,"Part Number=RESC0805 10K 1%",PCB3D=,"Pin Info=","Signal Integrity=",Simulation=,TCR=,"Temperature Max=","Temperature Min=",Tolerance=1%,Value=10k|CUSTOMPARAMETERS=
|RECORD=PartChoiceGroups|GROUPBYFIELDCOUNT=0
